
Instructions for PC Configuration Software

1. Ensure that the computer and the S3 are on the same local network;
2. Start the PC configuration software (Update & Configuration Tool). If the startup fails, choose to run it as a system administrator;
3. After starting the PC configuration software, select the device type as "CHTF-3.3", enter the access password "801801", and then click on "Search Device".(or S7, ‘801801’)



1. Click on the "Upload" button below, select the European firmware upgrade package (.bin file), then choose the device that needs to be upgraded, and finally click on the "Upgrade" button. After completion, a prompt will appear indicating a successful upgrade. (Note: If the upgrade not work, try to close you computer network firewall)

You can upgrade devices individually or in batches.

